=======================
 YAMAHA XGworks 3.0.7E
=======================

XGworks 3.0 is a powerful MIDI sequencer designed to fully support XG gear and software synths. Offering full control over the input and editing of MIDI & audio data, tone control, mixing, notation and so on, XGworks 3.0 is a complete XG-based sequencer solution that can form the heart of your PC music environment. 

XGworks 3.0 offers features not found in any other application of its kind, including dedicated XG editing support and full support of all XG parameters in the event list. No longer do you have to hunt through the pages of the user manual to understand the SysEx values or controller numbers being thrown at you, it is all displayed in plain English.

Features

- 100 track sequencing (MIDI, Wave, Style and Chord tracks) 
- Full editing (Quantize, etc) 
- Piano Roll Arranger 
- Guitar Arranger 
- Multi-Track Hard Disk Recording 
- Full XG Editing 
- Voice to Score - allows you to sing or hum a tune and XGworks 3.0 will convert it to musical score. 
- Staff Printing 
- Lyric input 
- Plug in module expansion 
- Full VL Support (for VL daughtercard, VL70m, MU100r) 
- Windows Standard shortcuts and Navigation 

System Requirements 

- Computer: IBM-PC/AT or compatible. 
- CPU: Pentium 75MHz or greater (Pentium 166MHz or greater is recommended). 
- OS: Windows 9x/Me/2k/XP. 
- System Memory: 16MB or more (32MB or more is recommended). 
- Hard disk: Minimum 40MB of free hard disk space. 
- Hardware: 
	- Soundcard with XG/XG software synthesis or MIDI interface for external module operation XG-compatible tone module or S-YXG50/S-YXG100 SoftSynthesizer.
	- MPC2 compliant sound card (such as DS-XG,WF192XG,SW1000XG) if using audio hard disk recording functions. 
- Software: Adobe Acrobat Reader should be installed to read the PDF manuals and books.

Specifications 

Number of Tracks: 100 tracks (MIDI/Wave tracks) + Style and Chord Tracks. 
Maximum Measures: 9,999. 
MIDI Ports: Maximum 6 ports. 
Audio Ports: Maximum 6 ports. 
MIDI channels: 1 - 16/port (Can be freely set for each MIDI track). 
Edit Windows: Track View Window, Piano Roll Window, Staff Window, Drum Window, List Window, Master Track Window, Mixer Window, XG Editor Window. 
Entry Format: Real-time recording, step recording (mouse, external MIDI keyboard), digital audio (wave) recording. 
Resolution: Quarter note = 480 ppqn. 
Compatible File Formats: Song files: XWS (XGworks Original File/XGworks Original File with Wave), MID (Standard MIDI File format 0/1 and XF file)
Wave (digital audio) files: WAV
XG parameter files: XGP (for Loading only), SYX (for Saving and Loading). 


XGworks Home Page: http://www.yamaha.co.uk/xg/html/midplug/m_mid10.htm

Copyright (C) 1996-2002 YAMAHA CORPORATION All Rights Reserved.


